50TON AIR SHOP PRESS
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FEATURE                                                                              MAINTENANCE         
1. Used for parts straightening, bending and pressing.                                             1.Periodically, lightly oil all moving parts including the pump piston and 

2. Multi-position bed for work height adjustment.                                                hydraulic ram.

3. With air pump can reduce labor and improve working efficiency                                  2.Check hydraulic connections and hoses before each use. Do not use 

OPERATION                                                                             if cut, damaged, leaking or otherwise damaged connections and/or 

	Part No.
	Description
	Qty
	Part No.
	Description
	Qty

	1
	Bolt
	6
	21
	Abor plate
	2

	2
	Cross beam
	1
	22
	Pressure beam
	1

	3
	Damping nut M16
	4
	23
	Jack
	1

	4
	Spring washer M22
	8
	24
	Bole
	4

	5
	Washer M22
	8
	25
	Washer M16
	8

	6
	Damping nut M22
	8
	26
	Gear
	1

	7
	Pole
	2
	27
	Gear seat 
	1

	8
	Pin
	2
	28
	Damping nut M10
	10

	9
	Tighter the scres
	4
	29
	Bole
	2

	10
	Washer M12
	38
	30
	Steel wire
	1

	11
	Bolt
	12
	31
	Collet
	2

	12
	Leg
	2
	32
	Steel shaft
	4

	13
	Damping nut M12
	6
	33
	Steel wheel
	4

	14
	Connect boart
	2
	34
	Washer M18
	4

	15
	Bolt
	7
	35
	Block loop
	4

	16
	Washer M10
	10
	
	
	

	17
	Bolt
	6
	
	
	

	18
	Pump
	1
	
	
	

	19
	Handle
	1
	
	
	

	20
	Adjust beam
	1
	
	
	


1. Place work piece on bed frame.                                                             hoses are noted

2. Locate and close release valve.

Pump handle until the ram nears work piece.                                               

4. Apply load to work piece by pumping handle. Do not overload work  

Piece.                                                                                                                                             
Remove load from work piece by turning release valve. Stabilize work                                                                                                                                   
piece so it does not fall while pressure is released.

6. Remove work piece after ram is fully retracted.                                                     
WARNING

This press is designed and intended for use by properly trained and 

experienced personnel only. If you are not familiar with the proper and                                                       
safe operation of a hydraulic press, do not use until proper training and 

knowledge has been obtained.

2. Do not operate this press beyond it rated capacity.

3. DO NOT compress springs or other objects that could be ejected from 

  the press. DO NOT compress objects that could shatter.

Check the press for loose or damaged parts before each operation. 

Replace damaged parts and tighten all loose bolts before operating.

Some parts being pressed may have a tendency to pop out of the press 

or explode under pressure. Protect yourself accordingly.  
